Version: 1.6.2.023

Basic features

* Support multiple devices processing.
* An independent process bar is setup for each physical USB port.
* Color based flag used to indicate users the status of the work:
* Blue indicates the device is being processed
* Green indicates the device was successfully processed, and indicates to tester it can be replaced with a fresh device independent of the other devices progress.
* Red indicates the device failed to process.
* Continuously monitors device removal/arrivals.
* It will automatically restart process when processed device is replaced with a new device
* Will start processing first device detected, and allows replacing each device after completion instead of waiting for all devices to complete.

Known issues

| **Identifier** | **Description** |
| --- | --- |
| ENGR126402 | No error message shows when VID/PID in ucl.xml is invalid. |
| ENGR126405 | "Configuration->General->Enable COM port status messages" is not supported. |
| ENGR131963 | "Configuration->Clean Registry..." is not work. |
| ENGR124632 | Windows prompt usb warning when in downloading and then stop download. |
| ENGR116918 | Performance measurement. |
| ENGR118075 | The progress bar of sending file is still going on after press "Stop" button. |
| ENGR118080 | MFGTool.exe crashes if unplug USB cable during sending FW. |